Open topic with navigation

# The Connector Summary Tab

To view a single connector in detail, click the connector in the navigation tree. The toolbar on the summary tab includes the following buttons for operations on the connector:

Connector Command | Sends a command to the connector. For more information, see Sending a Command to a Connector.
Remove Connector | Removes the connector. For more information, see Deleting a Connector .
Run Logfu | Run Logfu diagnostics on the connector. For more information, see Running Logfu on a Connector.
Share | Shares the connector through the ArcSight Marketplace. For more information, see Sharing Connectors in ArcSight Marketplace.

Tables below the toolbar show connector specifics, including basic connector data, parameters, and connector destinations. These tables include the following columns:

Connector Data

- Type: Type of connector.

- Status: Connector status.

- Input Events (SLC): Total number of events received by the connector since it was last checked (generally once per minute).

- Input EPS (SLC): Events per second received by the connector since it was last checked (generally once per minute).

- In addition, the columns to the right include tools for editing a connector, editing runtime parameters, adding a failover destination, and sending a destination command.

Connector Parameters

Click Connector Parameters to toggle display of this table. The Connector Parameters table includes:

- Click to edit parameters.

- Parameters: Parameters can include connector network port, IP address , protocol, and other information.

- Value: Parameter value.

Table Parameters (WUC Connectors Only)

WUC connectors (only) display these parameters.

- Domain Name: Connector domain name.

- Host Name: Connector host name.

- User Name: Connector user name.

- Security Logs: Indicates whether security events are collected.

- System Logs: Indicates whether system events are collected.

- Application: Indicates whether application events are collected from the Common Application Event Log.

- Custom Log Names: List of custom application log names, if any.

- Microsoft OS Version: Microsoft operating system for the connector.

- Locale: Connector locale.

Destinations

Click Destinations to toggle display of this table. The Destinations table includes:

- Click to add additional destinations.

- Name: Destination name.

- Output Events (SLC): Total number of events output by the connector to the destination since it was last checked (generally once per minute).

- Output EPS (SLC): Events per second output by the connector to the destination since it was last checked (generally once per minute).

- Cached: Total number of events cached to be transmitted to the destination.

- Type: Destination type. Destination types are described in the SmartConnector User's Guide.

- Location: Location of the destination.

- Device Location: Location of the device on which the destination is located.

- Comment: Comments on the destination.

- Parameters: Destination-specific parameters, such as IP address , port, and protocol.

- Action Buttons: Action buttons enable destination management tasks, such as editing the destination, editing the runtime parameters, adding a new failover destination, sending destination commands and removing the destination.

For more information on managing connectors, see Managing Connectors.