Open topic with navigation

# Configuring SmartConnector as a Transformation Hub Producer

Follow the steps in this section to configure a SmartConnector with a Transformation Hub destination with the encrypted security mode that you require. These procedures are provided with the following assumptions:

- You use the default password. To set a non-default password, see Password Management in the ArcSight SmartConnectors documentation.

- You are on the Linux platform. For Windows platforms, use backslashes (`\`) when entering commands instead of the forward slashes given here.

- You are using a command window to specify Windows commands. Do not use Windows PowerShell.

  In these instructions, `<th hostname>` refers to the FQDN hostname used to access the master node (for On-premisesor Azure installations) or, for AWS, the FQDN of the application load balancer; and <`th_port>` refers to either port 9092 (plain text) or 9093 (TLS)