Open topic with navigation

# Creating a Subscriber Configuration

You can create a subscriber configuration for pushing to any subscribed nodes.

Note: The following subscriber configuration types cannot be created in ArcMC, but can only be imported from managed nodes:

- Logger Storage Group

- Logger Filter

- Logger ESM Forwarder, Connector Forwarder, TCP Forwarder, UDP Forwarder

- Authentication External

For more information on importing a configuration from a managed node, see Importing a Subscriber Configuration.

To create a configuration:

1. Click Configuration Management > Subscriber Configurations > All Configurations.

   Tip: To filter for a specific subscriber configuration type, select the desired configuration type from the Subscriber Configurations sub-menu.

2. Under Configurations, click New.

3. On the Details tab, select a configuration type from the Configuration Type drop-down list. (Only the appropriate configuration types are shown in the drop-down list.)

4. In Configuration Name, enter a name for the configuration. (Configuration names must be unique and may be up to 255 characters in length.)

5. Enter values for any required parameters, which are indicated with a red asterisk (*).

   Note: For a description of valid parameters for each configuration type, and the data type associated with each, see Subscriber Configuration Types.

6. Optionally, add values for any optional parameters.

7. Optionally, to add an additional property for a list configuration: click Add Property, and then enter values for the prompted parameters. Repeat adding properties as needed to completely define the configuration.

8. Click Save.