Open topic with navigation

# Changing the Network Interface Address for Events

ArcMC has multiple network interfaces. By default, the connector determines which network interface address is used for events displayed in the ArcSight Console or Logger, but typically uses `eth0`.

To use a specific network interface address for events, add the parameter `connector.network.interface.name` to the Connector’s `agent.properties` file. For example, to use the IP address for `eth1`, specify the following parameter:

`connector.network.interface.name=eth1`