Content Manager 25.2 Content Manager

# Barcode scanner Connection tab

1. On the Manage tab, click Barcode Scanners.
2. Right-click an existing scanner and click Properties or right-click and click New Barcode Scanner to create a new one.
3. Click the Connection tab.
   - Process barcodes from file - select if you are reading previously scanned information from a file.

     For this option, you would download data from a barcode scanner to a file first and then use Content Manager to read the file.

   - Keyboard emulation or keyboard wedge device - select if you are downloading scanned labels through a keyboard Wedge.

     This device uses a computer's keyboard buffer.

   - Serial Communications - select if you connect the barcode scanner directly to the serial port.

   NOTE: For scanners that use the USB port, select the option Keyboard Emulation or keyboard wedge device and set the scanner to use keyboard emulation as per manufacturer's documentation.

   - Serial Port - select the serial port
   - Baud Rate - select the baud rate

     The majority of barcode scanners use 9600 baud.

     Data at the baud rate of 9600, 4800, 2400 or 1200 can be received.

   - Parity - select the applicable parity.

     The majority of barcode scanners use No Parity.

     See your barcode scanner reference manual for more information.

     The options are:

     - None
     - Odd
     - Even
   - Data Bits - select the applicable number of data bits.

     The majority of barcode scanners use 8 data bits.

     Transmission in 7 or 8 data bits is supported.

   - Stop Bits - select the applicable number of stop bits.

     The majority of barcode scanners use 1 stop bit.

     One or two stop bits are accepted.

   - Flow Control - select the applicable method of flow control.

     The majority of barcode scanners use either Xon/Xoff or RTS.

     You can use:

     - None

       NOTE: Setting a barcode scanner Flow Control to None does not work for batch downloads with any barcode scanner.

     - Xon/Xoff
     - RTS
     - Xon/RTS
   - Does scanner need acknowledgement character? - some barcode scanners require Content Manager to acknowledge that it received a barcode and must receive instructions to send the next one.

     Select if your barcode scanner requires this type of acknowledgement character.

   - Portable (batch download) - select if you are going to update your dataset by downloading a batch of scanned labels from a portable barcode scanner
   - Stationary (process immediately) - select if the barcode scanner will be connected to your computer during scanning and you want your dataset updated immediately when a barcode label is scanned
   - Timeout - set the timeout period so that the scanner dialogue box will close when no Activity has been detected within the period

See your barcode scanner reference manual for more information.

Copyright 2008-2025 Open Text
Version 25.2 | Last updated April 2025
Contact

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to hprmdocumentation@microfocus.com.

We appreciate your feedback!

Product: Content Manager 25.2

Topic Title: Barcode scanner Connection tab