Content Manager 25.2 Content Manager

# Barcode setup examples

Standard setup settings examples are listed below.

Portable settings

Barcode scanner name: | Portable
--- | ---
Does scanner send ID label first?: | Yes
Does scanner send EOF label at end? | Yes
Connection Method | Serial Communications
Serial Port | COM2
Parity | None
Data Bits | 8
Stop Bits | 1
Flow Control | RTS
Baud Rate | 9600
Download Method | Portable (batch download)

On-line settings

Barcode scanner name | Stationary
--- | ---
Does scanner send ID label first? | No
Does scanner send EOF label at end? | Yes
Connection Method | Serial Communications
Serial Port | COM2
Parity | None
Data Bits | 8
Stop Bits | 1
Flow Control | RTS
Baud Rate | 9600
Download Method | Stationary (process immediately)

Keyboard wedge settings

Barcode scanner name | Stationary (process immediately)
--- | ---
Does scanner send ID label first? | No
Does scanner send EOF label at end? | No
Connection Method | Keyboard Wedge
Download Method | Stationary (process immediately)

Copyright 2008-2025 Open Text
Version 25.2 | Last updated April 2025
Contact

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to hprmdocumentation@microfocus.com.

We appreciate your feedback!

Product: Content Manager 25.2

Topic Title: Barcode setup examples