Open topic with navigation

# FillGaps

Set `FillGaps` to `True`, if you want HPE Category Component to check if snapshots exist at the specified FillGapsFrequency intervals in the time span for which it generates the spectrograph. At any interval where no snapshot exists, HPE Category Component attempts to generate an additional snapshot to ensure that a spectrograph is generated without gaps.

Actions: | ClusterSGDataGen
Type: | Boolean
Default: | False
Example: | `FillGaps=True`
See Also: | FillGapsFrequency

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm