Open topic with navigation

# ScheduleInterval

The time between runs of this schedule. Set `ScheduleInterval` to the amount of time that must elapse after this schedule runs for the first time before it runs again. The default interval is `1 day`. Specify this value in the following format:

    NumberTimeUnit

where,

`Number` | The number of time units to elapse.
`TimeUnit` | The time unit to specify. The following units are available: second seconds minute minutes hour hours day days week weeks month months

NOTE:

If you do not specify a `timeUnit`, HPE Category Component reads the specified number as seconds.

The month time unit is 28 days.

Type: | String
Default: | 1 day
Required: | No
Configuration Section: | AnalysisSchedules
Example: | `ScheduleInterval=2 days`
See Also: | ScheduleAction ScheduleCycles ScheduleStartTime

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm