Open topic with navigation

# FillGapsFrequency

The interval (in seconds) at which HPE Category Component must check if snapshots exist in the timespan for which it generates the spectrograph. This option has an effect only when FillGaps is set to `True`. At any interval where no snapshot exists, HPE Category Component attempts to generate an additional snapshot to ensure that a spectrograph is generated without gaps.

Actions: | ClusterSGDataGen
Type: | Long
Default: | 86400
Example: | `FillGapsFrequency=43200`
See Also: | FillGaps

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm