Open topic with navigation

# UserAdd

Creates a new user in HPE Community Component.

## Example

    http://12.3.4.56:9000/action=UserAdd&UserName=Admin&Password=admpswd&FieldPhoneExt=077

This action uses port `9000` to add the `Administrator` user to HPE Community Component, which is situated on a machine with the IP address `12.3.4.56`. The `Admin` user password is `admpswd`, and they have a `PhoneExt` field associated with them that contains the value `077` (for example, a telephone extension).

## Parameters

Parameter | Description | Required
--- | --- | ---
EmailAddress | The e-mail address of the new user. |
FieldFieldName | A field to add to the user. |
InputEncoding | The encoding of the EmailAddress, Password, and UserName. |
OutputEncoding | The encoding to convert the results to. |
Password | The password for the new user. | Yes
RoleName | The name of the role to add the new user to. |
Security | A security field for the new user. |
UserName | The name of the new user. | Yes

This action accepts the following standard ACI action parameters.

Parameter | Description
--- | ---
ActionID | A string to use to identify an ACI action.
EncryptResponse | Encrypt the output.
FileName | The file to write output to.
ForceTemplateRefresh | Forces the server to load the template from disk.
Output | Writes output to a file.
ResponseFormat | The format of the action output.
Template | The template to use for the action output.
TemplateParamCSVs | A list of variables to use for the specified template.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm