Open topic with navigation

# TTL

The Time To Live of multicast IP packets for SSDP (that is. how many router hops are allowed). This defines the scope of an SSDP deployment.

Type: | Integer
Default: | 2
Required: | No
Configuration Section: | SSDP
Example: | `TTL=2`
See Also: |

© 2013 - 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm