Open topic with navigation

# SSLConfig

Identifies the configuration section in which the SSL configuration details are specified, usually `SSLOptionN`. You must set this parameter if you want to use SSL for communications between HPE Controller and other HPE products.

Set this parameter in the `[Server]` section of the HPE Controller configuration file to configure SSL for incoming ACI calls.

NOTE:

If you set `SSLConfig` for HPE Controller, all components that request licenses from HPE Controller must have a corresponding SSL configuration.

To configure components to communicate with HPE Controller using SSL, you must set `SSLConfig` in the `[License]` section of the server or component configuration file.

Type: | String
Default: | None
Required: | No
Configuration Section: | Server
Example: | `[Server] SSLConfig=SSLOption1 ... [AgentDRE] SSLConfig=SSLOption2 ... [DataDRE] SSLConfig=SSLOption2 ... // For Omni Group Servers: [Note] GroupServerHost=... GroupServerPort=... SSLConfig=SSLOption2 [SSLOption1] //SSL options for incoming connections SSLMethod=SSLV23 SSLCertificate=host1.crt SSLPrivateKey=host1.key SSLCACertificate=trusted.crt [SSLOption2] //SSL options for outgoing connections SSLMethod= SSLV23 SSLCertificate=host2.crt SSLPrivateKey=9s7BxMjD2d3M3t7awt/J8A SSLCACertificate=trusted.crt`
See Also: | Secure Socket Layer Parameters

© 2013 - 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm