Open topic with navigation

# Enabled

Whether SSDP is enabled. If SSDP is not enabled, the HPE Controller server is not included in the list of discovered HPE Controller servers in a `GetController` action sent to an HPE Coordinator. In addition, you can add the HPE Controller server to an HPE Coordinator only by specifying its port and IP address or host name, and not by specifying a UUID.

Type: | Boolean
Default: | True
Required: | No
Configuration Section: | SSDP
Example: | `Enabled=True`
See Also: |

© 2013 - 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm