Open topic with navigation

# ACI Encryption Configuration Parameters

You can encrypt communications between ACI servers (for example, HPE Controller and License Server) and any applications that use the HPE ACI API by configuring an `[ACIEncryption]` section in each of the application configuration files.

NOTE:

Instead of using ACI encryption, HPE recommends configuring Secure Socket Layer (SSL) connections between ACI servers and applications. For more information, see Secure Socket Layer Parameters.

For example:

    [ACIEncryption]
    CommsEncryptionType=GSS
    ServiceName=Kerberos

CommsAllowUnencrypted

CommsEncryptionType

ServiceName

See Also: Secure Socket Layer Parameters.

© 2013 - 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm