Open topic with navigation

# Port

The active port on which the Controller is running.

Actions: | AddController
Type: | Long
Default: | None
Required: | Yes, if you are using `IP` or `HostName` to specify the controller to add.
Example: | `Port=41200`
See Also: | IP HostName

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm