Open topic with navigation

# TimeoutMS

The time in milliseconds after which Coordinator stops trying to connect if there is no response from the Controller.

Type: | String
Default: | 25000
Required: | Yes
Configuration Section: | StatsCollector and Connection. If you set this parameter in the StatsCollector and Connection sections, the setting in the StatsCollector section takes precedence for statistics collection.
Example: | `TimeoutMS=25000`
See Also: |

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm