Open topic with navigation

# AddController

Adds a Controller to Coordinator. You can specify a Controller by UUID (Universal Unique ID), or by active host and port.

## Example

    http://123.4.5.67/action=AddController&UUID=d267cf80-063a-8030-a2de-24be0523821c

    http://123.4.5.67/action=AddController&HostName=localhost&Port=41200
    &ConnectByHostName=True

    http://123.4.5.67/action=AddController&IP=1.2.3.4&Port=41200

## Parameters

Parameter | Description | Required
--- | --- | ---
ConnectByHostName | Set to `True` if you want to add the Controller by specifying host name information. | Yes, if you are also using `HostName`.
HostName | The name of the active host on which the Controller is running. |
IP | The IP address of the machine on which the Controller is running. |
Port | The active port on which the Controller is running. | Yes, if you are using `IP` or `HostName`.
UseSSL | Specifies whether the Controller uses SSL. |
UUID | The UUID of the controller that you want to add. |

## Comments

You must set one of UUID, IP and Port, or HostName and Port. If you add a Controller using `HostName`, you must set `ConnectByHostName` to `True`.

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm