Open topic with navigation

# CommsEncryptionTEAKeys

DEPRECATED:

The `CommsEncryptionTEAKeys` configuration parameter is deprecated for HPE Distributed Action Handler version 10.8.0 and later. Instead of using ACI encryption, HPE recommends configuring Secure Socket Layer (SSL) connections between ACI servers and applications. For more information, see Secure Socket Layer Parameters.

The `CommsEncryptionTEAKeys` configuration parameter is still available for existing implementations, but it might be incompatible with new functionality. The parameter might be deleted in future.

The BTEA key to use for encryption. If you have set CommsEncryptionType to `TEA`, use `CommsEncryptionTEAKeys` to set the key that BTEA uses for its encryption algorithm. The key contains four 32 bit values, separated by commas.

Type: | Long
Default: |
Allowed Range: | Minimum: 0 Maximum: 2000000000
Recommended Range: | Minimum: 0 Maximum: 2000000000
Required: | No
Configuration Section: | ACIEncryption
Example: | `CommsEncryptionTEAKeys=123,456,789,123`
See Also: | CommsAllowUnencrypted CommsEncryptionType

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm