Open topic with navigation

# Configure Asynchronous Actions

You can use the DAH to distribute asynchronous actions to child servers in mirror mode. When you send an asynchronous action, the child server immediately returns a token and queues the action. To check the status of the action, you send the `QueueInfo` action with the token returned by the child server.

For details of asynchronous actions and the `QueueInfo` action, refer to the documentation for the server you are using.

To use HPE DAH to distribute asynchronous actions

- Add the `AsynchronousCommands` configuration parameter to the DAH configuration file.

  For example:

      [Server]
      AysnchronousCommands=ingest,tiff

  In this example, DAH distributes the `ingest` and `tiff` asynchronous actions to its child servers.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm