Open topic with navigation

# SSLConfig

Identifies the configuration section in which the SSL configuration details for distributed engines are specified, usually `SSLOptionN`. You must set this parameter if you are using SSL connections between HPE DAH and child engines.

Setting this parameter in the `[Server]` section controls incoming ACI calls.

Setting this parameter in the `[DistributedEngineN]` section controls outgoing ACI calls to child engines in a Standalone HPE DAH system.

Setting this parameter in the `[IDOLServerN]` section controls outgoing ACI calls to child engines in a HPE DAH system Integrated with IDOL.

Setting this parameter in the `[DAHEngineN]` section controls outgoing ACI calls to child engines in a HPE DAH system Integrated with IDOL in which HPE DAH and DIH child engines are configured separately.

NOTE:

You can set this parameter in the `[Server]` section alone, in `[DistributedEngineN]`, `[DAHEngineN]`, or `[IDOLServerN]` alone, or in both the `[Server]` and either `[DistributedEngineN]`, `[DAHEngineN]`, or `[IDOLServerN]` sections, depending on how you want to manage your connections.

If you create a server group by specifying a comma-separated list of host names in the Host parameter, you can use a single value for `SSLConfig` so that all child servers in the group use the same SSL details. Alternatively, you can use a comma-separated list to use different details for each mirrored child server. In this case, there must be the same number of values in `SSLConfig` as there are for Host.

Type: | String
Default: |
Required: | No
Configuration Section: | IDOLServer `N` or DistributedEngine `N` or DAHEngine `N`
Example: |
    [DistributedEngine0]
    SSLConfig=SSLOption0
In this example, the SSL connection to DistributedEngine0 is configured in the SSLOption0 section.
    ...
    [Server]
    SSLConfig=SSLOption

    [DistributionIDOLServers]
    Number=2

    [IDOLServer0]
    SSLConfig=SSLOption

    [IDOLServer1]
    SSLConfig=SSLOption1
In this example, incoming ACI calls and outgoing calls to IDOLServer0 use the same SSL configuration, but outgoing calls to IDOLServer1 use a different SSL configuration.
See Also: | Host Secure Socket Layer Parameters

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm