Open topic with navigation

# TimeBetweenRetries

The number of milliseconds that you want to elapse after the HPE Distributed Action Handler has checked down servers before it checks them again.

Type: | Long
Default: | 5000
Allowed Range: | Minimum: 100 Maximum: 86400000
Recommended Range: | Minimum: 100 Maximum: 60000
Required: | No
Configuration Section: | Server
Example: | `TimeBetweenRetries=240000` In this example, the HPE Distributed Action Handler waits 240,000 milliseconds (4 minutes) before it attempts to reconnect to an IDOL Server that is down.
See Also: |

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm