Open topic with navigation

# Host

The host name or IP address of the child server that the HPE Distributed Action Handler communicates with.

In non-mirror mode, you can also specify a comma-separated list of host names of mirrored child servers to create a child server group.

NOTE:

If you are using VDBs, you cannot also use server groups.

Type: | String
Default: |
Required: | Yes
Configuration Section: | IDOLServer `N` or DistributedEngine `N` or DAHEngine `N`
Example: | `Host=testserver1`
See Also: | Port Weight

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm