Open topic with navigation

# ServiceControlClients

The IP addresses or names of clients that can send service control actions to the service. Separate multiple addresses with commas. There must be no space before or after the comma.

Adding a client to `ServiceControlClients` does not enable it to send service status actions. To enable a client to send status actions, you must add the IP address or host name to the ServiceStatusClients.

You can use wildcards in the IP addresses. For example, type `187.*.*.*` to permit any machine whose IP address begins with `187` to control the service. You can also filter the `ServiceControlClients` parameter using CIDR notation.

Type: | String
Default: | None
Required: | Yes
Configuration Section: | Service
Example: | `ServiceControlClients=localhost,127.0.0.1`
See Also: | ServiceACIMode ServiceHost ServicePort ServiceStatusClients

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm