Open topic with navigation

# Send Minimal Documents

In non-mirror mode, you can configure HPE DIH to send each child server only the information it needs. In `DistributeSendMinimal` mode, the HPE DIH determines which child server must index each document, and sends the complete document only to that child server.

HPE DIH sends a minimal representation of the document to all other child servers. The content of this representation is defined by the `KillDuplicates` mode of the original index action.

This mode allows all child servers to perform correct deduplication, and reduces network traffic to child servers.

To enable minimal sending mode, set the `DistributeSendMinimal` configuration parameter to `True` in the `[Server]` section. For example:

    [Server]
    MirrorMode=False
    DistributeSendMinimal=True

NOTE:

When you want to deduplicate on a field other than `DREREFERENCE`, you must configure a field process in the DIH configuration file, with the fields that you want to use to deduplicate. DIH then includes these fields in the representation that it sends to its child servers. By default, it sends only the `DREREFERENCE`.

For more information about setting up a field process, refer to the IDOL Server Administration Guide.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm