Open topic with navigation

# Threads

The maximum number of parallel listening threads for index actions.

Set this parameter to the number of index actions that the server can receive at the same time. HPE DIH queues these actions, and processes the queue using a single processing thread.

You can calculate the optimum number of threads as follows:

(1 x Num CPU's) + 1 spare thread.

The optimum number of threads also depends on the number of clients sending index actions to HPE DIH. For example, if you have only one CFS sending index actions to HPE DIH, you need only one thread.

Type: | Long
Default: | 10
Recommended Range: | Minimum: 4 Maximum: 32
Required: | No
Configuration Section: | IndexServer
Example: | `Threads=2`
See Also: |

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm