Open topic with navigation

# IngestRate

The rate at which HPE Media Server ingests video.

You must use `IngestRate=1` for streams and in most cases HPE recommends `IngestRate=0` for video files.

The parameter accepts the following values:

- `1` - HPE Media Server ingests video at normal (playback) speed. Assuming there are no external limitations such as network bandwidth, HPE Media Server ingests one minute of video every minute. If an analysis task cannot process frames at this rate, it will analyze fewer frames.

- `0` - The rate at which video is ingested is determined by the slowest analysis task that you have configured. Some analysis tasks are very fast, but some are slower and can analyze only one or two frames per second per thread. With `IngestRate=0`, the amount of time required to ingest a video file depends on the analysis tasks that you have configured and the resources available to HPE Media Server.

  NOTE:

  Even with `IngestRate=0`, HPE Media Server does not analyze every frame. The number of frames that are analyzed depends on the value of the configuration parameter `SampleInterval`, which you can configure for most analysis tasks. If you want to analyze every frame of a video file, you must set `IngestRate=0` and then set `SampleInterval=0` for all relevant analysis tasks. However, HPE does not recommend processing every frame because in most cases this will take far longer and may not increase accuracy.

Options | Default SampleInterval | SampleInterval = 0
IngestRate=1 | HPE recommends using `IngestRate=1` and the default sample intervals for processing live streams. HPE Media Server does not attempt to process every frame, but selects frames for analysis based on the specified sample interval. The default sample intervals should provide good accuracy in most cases. If necessary, HPE Media Server will increase the sample interval to ensure that analysis occurs at normal (playback) speed. If HPE Media Server does not have sufficient resources, it will increase the sample interval, which might cause a reduction in accuracy. | HPE Media Server attempts to analyze every frame, but frames are skipped if the analysis tasks you have configured cannot process the frames at normal (playback) speed. HPE does not recommend these settings because processing every frame is usually not necessary and HPE Media Server is likely to skip large numbers of frames.
IngestRate=0 | HPE recommends `IngestRate=0` and the default sample intervals for processing video from files. HPE Media Server does not attempt to process every frame, but selects frames for analysis based on the specified sample interval. The default sample intervals should provide good accuracy in most cases. If analysis is slow, HPE Media Server ingests the file at a slower rate so that frames can be analyzed at the requested sample interval. If HPE Media Server does not have sufficient resources, it will take longer to process the file, but accuracy is maintained. | Ensures that all frames are analyzed. HPE does not recommend these settings because in most cases this will take much longer and might not increase accuracy. Use this mode only if it is critical that every frame is analyzed.

Type: | Number
Default: | 1
Required: | No
Configuration Section: | Ingest
Example: | `IngestRate=0`
See Also: |

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm