Open topic with navigation

# Configure Keyframe Extraction

To extract keyframes from video

1. Create a new configuration to send to HPE Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Analysis]` section, add a new analysis task by setting the `AnalysisEngineN` parameter. You can give the task any name, for example:

       [Analysis]
       AnalysisEngine0=Keyframes

3. Create a new configuration section to contain the task settings, and set the following parameters:

   `Type` | The analysis engine to use. Set this parameter to `keyframe`.
   `Input` | (Optional) The name of the image track to process.
   `ForceAfter` | (Optional) The maximum time interval between keyframes.
   `QuietPeriod` | (Optional) The minimum time interval between keyframes.
   `Sensitivity` | (Optional) The sensitivity of the engine to scene changes.

   For example:

       [Keyframes]
       Type=keyframe
       Sensitivity=0.6
       ForceAfter=5minutes

   For more information about the parameters that you can use to configure this task, refer to the HPE Media Server Reference.

4. Save and close the configuration file. HPE recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm