Open topic with navigation

# RecorderPort

The TCP port of the XProtect recording server. HPE Media Server receives video from the recording server.

Type: | Integer
Default: | If SOAPAuthentication is set to `false`, or the engine detects that it has logged on to an XProtect Enterprise system, the default value is `80`. If SOAPAuthentication is set to `true` and the engine detects that it has logged on to an XProtect Corporate system, the default value is `7563`.
Required: | No
Configuration Section: | TaskName
Example: | `RecorderPort=7563`
See Also: | RecorderHost

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm