Open topic with navigation

# Border

The amount of padding to add to the supplied region, before cropping the image. If the amount of padding that you specify extends beyond the boundary of the original image, HPE Media Server adds padding up to that limit and does not add blank space.

Specify the value in the units specified by BorderUnit.

Type: | String
Default: | 0
Required: | No
Configuration Section: | TaskName
Example: | `Border=5`
See Also: | BorderUnit

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm