Open topic with navigation

# Ingest MJPEG Video streamed over HTTP

This section describes how to ingest MJPEG video that is streamed over HTTP.

To ingest MJPEG video that is streamed over HTTP

1. Create a new configuration to send to HPE Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Ingest]` section, set the following configuration parameters:

   `IngestEngine` | The name of a section in the configuration file that will contain the ingestion settings.

   For example:

       [Ingest]
       IngestEngine=MJPEG

3. Create a new section in the configuration file to contain the ingestion settings, and set the following parameters:

   `Type` | The ingest engine to use. Set this parameter to `MJPEG_HTTP`.

   For example:

       [MJPEG]
       Type=MJPEG_HTTP

   TIP:

   There is no configuration parameter to specify the source. You must specify the URL of the stream that you want to ingest as the value of the `Source` parameter in the `Process` action, when you start processing.

   For more information about the parameters you can set to configure ingestion, refer to the HPE Media Server Reference.

4. Save and close the configuration file. HPE recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm