Open topic with navigation

# MinTimeInterval

The minimum time in milliseconds between a record in the first track and a record in the second track, for the record in the first track to be included in the output. Records from the second track are never included in the output.

NOTE:

This parameter is used only when you process video. When you process images or documents, this parameter is ignored and records are considered to be related only if they are associated with the same page.

Type: | Integer
Default: | 0
Required: | No
Configuration Section: | TaskName
Example: | `MinTimeInterval=0`
See Also: |

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm