Open topic with navigation

# Send Actions to HPE Media Server

You can make requests to HPE Media Server by using either GET or POST HTTP request methods.

- A GET request sends parameter-value pairs in the request URL. GET requests are appropriate for sending actions that retrieve information from HPE Media Server, such as the `GetStatus` action. For more information, see Send Actions by Using a GET Method.
- A POST request sends parameter-value pairs in the HTTP message body of the request. POST requests are appropriate for sending data to HPE Media Server. In particular, you must use POST requests to upload and send files to HPE Media Server. For more information, see Send Data by Using a POST Method.

HPE recommends that you send video data to HPE Media Server by providing a URL or a path to a file. Video files are very large and sending them over HTTP, as either multipart/form-data or a base64 encoded string, could cause HPE Media Server to slow and potentially lead to interruptions in service. Image, audio, and text files are generally much smaller and so you can send these files over HTTP.

NOTE:

HPE Media Server accepts HTTP strings that contain a maximum of 64,000 characters, and uploaded files with a maximum size of 10,000,000 bytes. You can override the default settings by setting the `MaxInputString` and `MaxFileUploadSize` configuration parameters in the `[Server]` section of the configuration file.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm