Open topic with navigation

# AndNotThen Engine Configuration Parameters

An AndNotThen engine compares two tracks and produces a track containing records from the first track for events that are not followed within a specified time interval by events in the second track. This section describes the parameters that you can set in the configuration section for an AndNotThen ESP task.

Configuration Parameter | Description
--- | ---
Input0 | The first input track.
Input1 | The second input track.
LuaScript | A Lua script that defines conditions for a discarding a record from the first track.
MaxTimeInterval | The maximum interval from the first track's record to the second track's record, for the two records to be considered a pair. (The AndNot engine discards record pairs.)
MinTimeInterval | The minimum interval from the first track's record to the second track's record, for the two records to be considered a pair. (The AndNot engine discards record pairs.)
Type | The type of ESP engine to use. Set this parameter to `AndNotThen`.

## Output Tracks

This engine produces a single output track, named `TaskName.Output`.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm