Open topic with navigation

# MinTimeInterval

The minimum time in milliseconds from a record in the first track to a record in the second track, for the two records to be considered a pair. (The engine compares the timestamp values.)

Type: | Integer
Default: | 0 (zero)
Required: | No
Configuration Section: | TaskName
Example: | `MinTimeInterval=100`
See Also: |

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm