Open topic with navigation

# QuietPeriod

The minimum time interval between keyframes. After identifying a keyframe, the engine does not identify another keyframe until after the specified time has elapsed, even if the scene changes.

Type: | Time Duration The value of this parameter is a time duration. Specify the duration in the following format:
         1years 2months 3weeks 4days 5hours 6minutes 7.8seconds
You can omit any of the individual durations when they are not required:
         6minutes 7seconds
You can also shorten the string by abbreviating the units to their first letter (months abbreviates to m, minutes to n):
         6n 7s
If you want to specify the value in seconds, no units are required:
         60
The following are all equivalent:
         1minute 3seconds
         1n 3s
         63s
         63
Default: | 1
Required: | No
Configuration Section: | TaskName
Example: | `QuietPeriod=5seconds`
See Also: | ForceAfter

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm