Open topic with navigation

# Pre-Allocate Storage for a Rolling Buffer

HPE Media Server must allocate storage for a rolling buffer before it can write encoded video to the buffer. Allocating storage is not instantaneous so to ensure that HPE Media Server can start recording from a stream immediately, pre-allocate storage before you start a session.

To pre-allocate storage in the rolling buffer

- Send the `PreAllocateStorage` action to HPE Media Server:

  `http://localhost:14000/action=PreAllocateStorage`

  For more information about this action, refer to the HPE Media Server Reference.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm