Open topic with navigation

# StreamTimeout

The number of seconds that HPE Media Server waits for the next record from a stream. If a record is not received from Milestone XProtect within this time, HPE Media Server stops ingesting the source.

TIP:

If a timeout occurs but you started processing with the Persist action parameter set to `TRUE`, HPE Media Server will attempt to reconnect to Milestone XProtect.

Type: | Integer
Default: | 60
Required: | No
Configuration Section: | TaskName
Example: | `StreamTimeout=30`
See Also: |

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm