Open topic with navigation

# Classify Images

To classify images or video frames

1. Create a new configuration to send to HPE Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Analysis]` section, add a new analysis task by setting the `AnalysisEngineN` parameter. You can give the task any name, for example:

       [Analysis]
       AnalysisEngine0=Classification

3. Create a new configuration section to contain the task settings, and set the following parameters:

   `Type` | The analysis engine to use. Set this parameter to `ObjectClass`.
   `Input` | (Optional) The image track to process. If you do not specify an input track, HPE Media Server processes the first track of the correct type that is produced by the ingest engine.
   `Classifier` | The classifier to use for classification. HPE Media Server categorizes objects into the classes in this classifier.
   `ClassificationThreshold` | (Optional) The minimum confidence score necessary for HPE Media Server to output a classification result. Any classification result with a confidence score below the threshold is discarded.

   For example:

       [Classification]
       Type=ObjectClass
       Classifier=Vechicles
       ClassificationThreshold=15

   For more information about these parameters, refer to the HPE Media Server Reference.

4. Save and close the configuration file. HPE recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm