Open topic with navigation

# UserClients

One or more IP addresses for machines that are permitted to send user commands to the `Port`. Separate multiple addresses using commas (there must be no space before or after a comma).

You can use wildcards in the IP addresses. For example, type `187.*.*.*` to permit any machine whose IP address begins with `187` to access the service's status. You can also filter the `UserClients` parameter using CIDR notation.

Type: | String
Default: | *.*.*.*
Required: | No
Configuration Section: | [Server]
Example: | `UserClients=12.34.56.7,2.4.6.8`
See Also: | AdminClients Port

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm