Open topic with navigation

# SectionerMinBytes

The minimum number of bytes recommended for a section. This is not a hard limit, but section sizes are generally kept above this.

Type: | Integer
Default: | `SectionerMaxBytes / 2`
Required | No
Configuration Section: | The configured section or Sectioning
Example: | `SectionerMinBytes=1500`
See Also: | SectionerMaxBytes

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm