Open topic with navigation

# MediaServerTimeout

The maximum amount of time that HPE CFS should wait for Media Server to respond, in seconds.

Type: | Integer
Default: | 60
Required | No
Configuration Section: | Any section that you have defined for media analysis task settings
Example: | `MediaAnalysisTimeout=40`
See Also: |

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm