Open topic with navigation

# MediaServerHost

A comma-separated list of Media Servers to use for running analysis on media. Specify the host name and ACI port for each Media Server, separated by a colon (`:`). HPE CFS distributes requests between the specified servers.

Alternate Name: | MediaServerHosts
Type: | String
Default: |
Required | Yes
Configuration Section: | Any section that you have defined for media analysis task settings
Example: | To use a single Media Server for analysis: `MediaServerHost=server1:14000` To use more than one Media Server, specify the servers in a comma-separated list: `MediaServerHost=server1:14000,server2:14000`
See Also: |

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm