Open topic with navigation

# EngineCheckTimeout

The timeout (in seconds) for when HPE Distributed Action Handler connects to and checks the configuration of the child servers during startup.

Type: | Long
Default: | 10
Allowed Range: | Minimum: 1 Maximum: 600
Recommended Range: | Minimum: 1 Maximum: 60
Required: | No
Configuration Section: | Server
Example: | `EngineCheckTimeout=30`
See Also: | EngineTimeout PingTimeout

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm