Open topic with navigation

# PeriodInDay

The time in days dedicated for indexing data on each child server, after the first roll over has occurred. At the end of this period, a DREINITIAL index action is sent to the next server and ACI requests are sent to the DAH to power up or power down the appropriate child servers.

If you do not use this parameter, then you must use PeriodInSec to set a period.

NOTE:

If you use this parameter, then you must set NextServerStartTime=`00:00`.

Type: | Long
Default: |
Required: | No
Configuration Section: | RoundRobinMode
Example: | `PeriodInDay=1`
See Also: | PeriodInSec NextServerStartTime

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm