Open topic with navigation

# AdminClients

The `AdminClients` parameter specifies the IP addresses (or host names) of clients that are permitted to send administrative commands to the ACI Port. Separate multiple addresses with commas. There must be no space before or after the comma.

You can use wildcards in the IP address. For example, `187.*.*.*` includes any machine with an IP address that starts with `187`. You can also filter the `AdminClients` parameter using CIDR notation.

NOTE:

Adding a client to `AdminClients` does not enable it to send service actions. To enable a client to send service actions, you must add the IP address or host name to the ServiceControlClients or ServiceStatusClients.

You can also configure client permissions by using the `[AuthorizationRoles]` configuration section. This section provides a more flexible method for setting up user authorization, and also allows you to set up permissions by using SSL identities or GSS principals. See Authorization Roles Configuration Parameters.

Configuring an authorization role with StandardRoles set to `Admin` overrides the default value for `AdminClients`.

To disable authorization by client IP address, set this parameter to `""`. In this case, HPE Eduction Server uses the options that you set in the `[AuthorizationRoles]` section only.

Type: | String
Default: | `localhost`
Required: | No
Configuration Section: | Server
Example: | `AdminClients=localhost,196.172.87.11`
See Also: | QueryClients

© 2014-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm