Open topic with navigation

# Service Configuration Parameters

This section describes the Service configuration parameters that determine which machines are permitted to use and control a service.

Access-Control-Allow-Origin

FIPSMode

ServiceACIMode

ServiceControlClients

ServiceHost

ServicePort

ServiceStatusClients

SSLConfig

TCPReceiveWindowSize

XSLTemplates

You must enable the service port by specifying the ServicePort, ServiceStatusClients, and ServiceControlClients configuration parameters.The service port then accepts the standard status and control actions described in Service Actions.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm