Open topic with navigation

# MaxConsecutiveTries

The maximum number of attempts that HPE Media Server makes to connect to the servers listed in the LanguageIDServers parameter.

If `MaxConsecutiveTries` is set to `0`, HPE Media Server continues attempting to connect to the IDOL Speech Servers indefinitely.

During live ingest, HPE recommends setting `MaxConsecutiveTries` to `0` so that the session is not stopped. When ingesting files, you might want the session to fail immediately so that another component can try to process the file on a different HPE Media Server and IDOL Speech Server setup.

Type: | Integer
Default: | 0
Required: | No
Configuration Section: | TaskName
Example: | `MaxConsecutiveTries=2`
See Also: | ErrorMessage

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm