Open topic with navigation

# View the Rolling Buffer Contents

To retrieve a list of all the rolling buffers that have been configured use the following procedure.

To list your rolling buffers

- Send the `GetStreams` action to HPE Media Server. For example:

      http://localhost:14000/action=GetStreams

  HPE Media Server returns a list of all of your rolling buffers.

You can also retrieve information about the video stored in a rolling buffer. For example, you might record video for one hour each morning and two hours each afternoon. To get information about what has been stored in a rolling buffer, use the following procedure.

To return a list of the content in a rolling buffer

- Send the `GetRecordedRanges` action to HPE Media Server.

  You can filter the results by setting the following optional parameters:

  `Stream` | The rolling buffer to list of recorded content for. If this parameter is not set, HPE Media Server returns results for all rolling buffers.
  `StartTime` | Only show content available after this time. Specify the start time in epoch milliseconds or ISO-8601 format.
  `Duration` | The length of time after the start time to return a list of available content for. Specify the duration as a time duration.

  For example, to retrieve a list of content available in the `BBCNews` rolling buffer for 24 hours from 16:27:54 on 21 February 2014:

      http://localhost:14000/action=GetRecordedRanges&Stream=BBCNews
                                                     &StartTime=1393000074243
                                                     &Duration=24hours

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm