Open topic with navigation

# Start and Stop Processing

This section describes how to start and stop processing, when you have chosen to split processing between multiple HPE Media Servers.

To start processing

- Start processing as described in Start Processing. Send the `Process` action to the upstream HPE Media Server only. You can use the `Config`, `ConfigName`, or `ConfigPath` action parameter to specify the configuration for the upstream HPE Media Server.

  The upstream HPE Media Server automatically starts a session on the downstream HPE Media Server.

To stop processing

- Stop processing as described in Stop Processing. Send the `QueueInfo` action to the upstream HPE Media Server only.

  The upstream HPE Media Server automatically stops the session on the downstream HPE Media Server.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm