Open topic with navigation

# Configure the Downstream Media Server

This section describes how to configure HPE Media Server to receive records from another HPE Media Server and continue processing them.

To receive records from another HPE Media Server

1. Create a new configuration file, or open an existing configuration that you want to modify.

2. In the `[Ingest]` section, add a new ingest task by setting the `IngestEngineN` parameter. You can give the task any name, for example:

       [Ingest]
       IngestEngine=RecordsFromUpstream

3. Below the `[Ingest]` section, create a new configuration section by typing the task name inside square brackets. For example:

       [RecordsFromUpstream]

4. In the new section, set the following parameters:

   `Type` | The ingest engine to use. Set this parameter to `Receive`.
   `Input` | A comma-separated list of tracks to receive from the other HPE Media Server.

   For example:

       [RecordsFromUpstream]
       Type=Receive
       Input=FaceDetect.ResultWithSource
       // or using alias "DetectedFaces", if defined in upstream configuration:
       // Input=DetectedFaces

5. Configure the analysis, encoding, ESP, and output tasks that you want to run on the ingested records.

   NOTE:

   The tracks produced by the `Receive` engine are prefixed with the name of the ingest task. For example, if you use the configuration above the track produced by the `Receive` engine is named:

   - `RecordsFromUpstream.FaceDetect.ResultWithSource` (if no alias is defined).
   - `RecordsFromUpstream.DetectedFaces` (if the alias `DetectedFaces` is defined by the upstream HPE Media Server).

   You must use the correct track name for the input of your face recognition task on the downstream HPE Media Server.

6. Save the configuration file in the location specified by the `ConfigDirectory` parameter.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm